**Section 215.245 Transfer of Liquids**

a) A competent attendant shall supervise the transfer of liquids from the time the connections are first made until they are disconnected.

b) Pumps shall be of a material suitable for use with the solution being handled and designed to withstand the working pressure.

c) Air compressors may be used for transfer of nitrogen fertilizer solutions.

1) The air compressor shall be protected with a back flow check valve in the air line to prevent the flow of nitrogen fertilizer solutions or vapor from the container into the air compressor.

2) A relief valve large enough to discharge the full capacity of the compressor shall be connected to the discharge before any shutoff valve.

d) All storage installations shall be equipped with devices so as to minimize tampering while installation is unattended.

e) Containers shall be filled or used only upon authorization of owner or owner's agent.