**Section 433.455 Access to Sub-Systems**

The operating and or security sub-system shall be accessible from no more than two terminals at any one point in time. These terminals shall be located in the tote room and access to these sub-systems shall require pass word entry prior to execution.