**Section 1316.60 Starting Gate Shields**

The arms of all starting gates shall be provided with a screen or a shield in front of the position for each horse, and such arms shall be perpendicular to the rail.