**Section 1440.70 Photo-Finish Camera**

All tracks conducting quarter horse meets must be equipped with a photo finish timing camera which has electronic circuits and a quartz crystal timing base and must be capable of operating either AC or DC without loss of accuracy. Every camera must be calibrated and accurate to a minimum of 1/100th of a second.