**Section 315.120 Additional Requirements for Optical Fiber Communications Systems**

a) Laser communication systems that employ optical cables shall be considered enclosed systems with the optical cable forming part of the protective housing.

b) Disconnection of a connector resulting in access to radiation in excess of the applicable MPE shall take place only in a controlled area.

1) The use of a tool shall be required for the disconnection of a connector for service and maintenance purposes when the connector is not within a protective housing.

2) All connectors shall bear the appropriate label specified in Section 315.150 of this Part.