**Section 351.1100 Inspection and Maintenance**

a) Each licensee or registrant shall conduct, at intervals not to exceed6 months, a program of inspection and maintenance of source holders, logging tools, source handling tools, storage containers, transport containers and injection tools to assure proper labeling and physical condition. Records of inspection and maintenance shall be maintained for a period of 2 years for inspection by the Agency.

b) If any inspection conducted pursuant to subsection (a) of this Section reveals damage to labeling or components that could result in release of radioactive material into the environment, or loss of control of radioactive material or that could otherwise create a risk of increase in radiation exposure, the device shall be removed from service until repairs have been made.

c) The repair, opening or modification of any sealed source shall be performed only by persons specifically authorized to do so by the Agency, the U.S. Nuclear Regulatory Commission, an Agreement State or a Licensing State.

(Source: Amended at 28 Ill. Reg. 12643, effective October 1, 2004)