**Section 351.530 Energy Compensation Source (ECS)**

a) The licensee may use an ECS that is contained within a logging tool, or other tool components only if the ECS contains quantities of licensed material not exceeding 3.7 MBq (100 microCi).

b) For well logging applications with a surface casing for protecting fresh water aquifers, use of the ECS is only subject to the requirements of Sections 351.350, 351.370, and 351.390.

c) For well logging applications without a surface casing for protecting fresh water aquifers, use of the ECS is subject to the requirements of Sections 351.150, 351.350, 351.370, 351.390, 351.510, and 351.770.