**Section 422.APPENDIX C Radon and Radon Decay Product Measurement Method Categories**

|  |  |  |  |
| --- | --- | --- | --- |
| A | (pCi/L) | B | (WL) |
|  |  |  |  |
| AC | Activated charcoal adsorption integrating |  |  |
|  |  |  |  |
| AT | Alpha track detection | CW | Continuous working level monitor |
|  |  |  |  |
| LS | Charcoal liquid scintillation |  |  |
|  |  |  |  |
| CR | Continuous radon monitor |  |  |
|  |  |  |  |
| EL | Electret ion chamber; long-term |  |  |
|  |  |  |  |
| ES | Electret ion chamber; short-term |  |  |

(Source: Amended at 33 Ill. Reg. 14479, effective October 9, 2009)