**Section 211.330 Air Dried Coatings**

"Air dried coatings" means any coatings that dry by use of air or forced air at temperatures up to 363.15º K (194º F).

(Source: Added at 17 Ill. Reg. 16504, effective September 27, 1993)