**Section 211.470 Air Assisted Airless Spray**

"Air assisted airless spray" means a spray coating method which combines compressed air with hydraulic pressure to atomize the coating material into finer droplets than is achieved with pure airless spray. Lower hydraulic pressure is used than with airless spray.

(Source: Added at 17 Ill. Reg. 16504, effective September 27, 1993)