**Section 211.2970 High Temperature Aluminum Coating**

"High temperature aluminum coating" means a coating that is certified to withstand a temperature of 537.8° C (1000° F) for 24 hours.

(Source: Added at 17 Ill. Reg. 16504, effective September 27, 1993)