**Section 212.202 Emission Units For Which Construction or Modification Commenced Prior to April 14, 1972, Using Solid Fuel Exclusively Located Outside the Chicago Area**

No person shall cause or allow the emission of particulate matter into the atmosphere from any fuel combustion emission unit for which construction or modification commenced prior to April 14, 1972, using solid fuel exclusively, which is located outside the Chicago major metropolitan area, to exceed the limitations specified in the table below in any one hour period except as provided in Section 212.203 of this Subpart.

|  |  |
| --- | --- |
| METRIC UNITS | |
|  |  |
| H (Range) | S |
| MW | Kg/MW |
|  |  |
| Less than or equal to 2.93 | 1.55 |
|  |  |
| Greater than 2.93 but smaller than 73.2 | 3.33 H-0.715 |
|  |  |
| Greater than or equal to 73.2 | 0.155 |

|  |  |
| --- | --- |
| ENGLISH UNITS | |
|  |  |
| H (Range) | S |
| mmbtu/hr | lbs/mmbtu |
|  |  |
| Less than or equal to 10 | 1.0 |
|  |  |
| Greater than 10 but smaller than 250 | 5.18H-0.715 |
|  |  |
| Greater than or equal to 250 | 0.1 |

where:

|  |  |  |
| --- | --- | --- |
| S | = | Allowable emission standard in lbs/mmbtu/hr or kg/MW of actual heat input, and |
| H | = | Actual heat input in mmbtu/hr or MW-hr |

(Source: Amended at 20 Ill. Reg. 7605, effective May 22, 1996)