**Section 214.303 Use of Sulfuric Acid**

With the exception of fuel combustion emission sources and acid manufacturing, no person using sulfuric acid shall cause or allow the emission of sulfuric acid and/or sulfur trioxide from all other similar emission sources at a plant or premises to exceed:

a) 45.4 grams in any one hour period for sulfuric acid usage less than 1180 Mg/yr (100 percent acid basis) (0.10 lbs/hr up to 1300 T/yr);

b) 250 grams per metric ton of acid used for sulfuric acid usage greater than or equal to 1180 Mg/yr (100 percent acid basis) (0.50 lbs/T over 1300 T/yr).

(Source: Amended at 7 Ill. Reg. 4219, effective March 28, 1983)