**Section 215.926 Control Requirements**

a) Every owner or operator of an emission source of volatile organic material shall operate in compliance with RACT, which for emission sources subject to this Subpart shall be:

1) Emission capture and control techniques which achieve an overall reduction in uncontrolled volatile organic material emissions of at least 81%; or

2) For coating lines, volatile organic material emissions not to exceed 0.42 kg/l (3.5 lb/gal) of coating materials as applied, excluding water and any compounds which are specifically exempted from the definition of volatile organic material, on a daily basis. Owners and operators complying with this subsection are not required to comply with Section 215.301; or

3) An adjusted RACT emissions limitation obtained pursuant to Subpart I.

b) Owners and operators of emission sources subject to this Subpart shall comply with its requirements by April 1, 1989.

(Source: Added at 12 Ill. Reg. 7311, effective April 8, 1988)