**Section 219.445 Leaks: General Requirements**

The owner or operator of a petroleum refinery shall:

a) Develop a monitoring program plan consistent with the provisions of Section 219.446 of this Part;

b) Conduct a monitoring program consistent with the provisions of Section 219.447 of this Part;

c)) Record all leaking components which have a volatile organic material concentration exceeding 10,000 ppm consistent with the provisions of Section 219.448 of this Part;

d) Identify each component consistent with the monitoring program plan submitted pursuant to Section 219.446 of this Part;

e) Repair and retest the leaking components as soon as possible within 22 days after the leak is found, but no later than June 1 for the purposes of Section 219.447(a)(1) of this Part, unless the leaking components cannot be repaired until the unit is shut down for turnaround; and

f) Report to the Agency consistent with the provisions of Section 219.449 of this Part.

(Source: Amended at 17 Ill. Reg. 16918, effective September 27, 1993)