**Section 219.902 Testing Requirements**

a) Testing to demonstrate compliance with the requirements of this Subpart shall be conducted by the owner or operator by May 1, 2012. Thereafter, testing shall be conducted within 90 days after a request by the Agency, or as otherwise provided in this Subpart. The testing shall be conducted at the expense of the owner or operator and the owner or operator shall notify the Agency in writing 30 days in advance of conducting the testing to allow the Agency to be present during testing.

b) Testing to demonstrate compliance with the VOM content limitations in Section 219.901(b) of this Subpart shall be conducted as follows:

1) Method 24, incorporated by reference in Section 219.112 of this Part, shall be used for non-reactive adhesives. If it is demonstrated to the satisfaction of the Agency and the USEPA that plant adhesive formulation data are equivalent to Method 24 results, formulation data may be used. In the event of any inconsistency between a Method 24 test and a facility's formulation data, the Method 24 test will govern;

2) Appendix A of 40 CFR 63, Subpart PPPP, incorporated by reference in Section 219.112 of this Part, shall be used for reactive adhesives;

3) The manufacturer's specifications for VOM content for adhesives may be used if the specifications are based on results of tests of the VOM content conducted in accordance with methods specified in subsections (b)(1) and (b)(2) of this Section, as applicable.

c) For afterburners and carbon adsorbers, the methods and procedures of Section 219.105(d) through (f) of this Part shall be used for testing to demonstrate compliance with the requirements of Section 219.901(d) of this Subpart, as follows:

1) To select the sampling sites, Method 1 or 1A, as appropriate, 40 CFR 60, appendix A, incorporated by reference in Section 219.112 of this Part;

2) To determine the volumetric flow rate of the exhaust stream, Method 2, 2A, 2C, or 2D, as appropriate, 40 CFR 60, appendix A, incorporated by reference in Section 219.112 of this Part;

3) To determine the VOM concentration of the exhaust stream entering and exiting the emissions control system, Method 25 or 25A, as appropriate, 40 CFR 60, appendix A, incorporated by reference in Section 219.112 of this Part. For thermal and catalytic afterburners, Method 25 must be used, except under the following circumstances, in which case Method 25A must be used:

A) The allowable outlet concentration of VOM from the emissions control system is less than 50 ppmv, as carbon;

B) The VOM concentration at the inlet of the emissions control system and the required level of control result in exhaust concentrations of VOM of 50 ppmv, or less, as carbon;

C) Due to the high efficiency of the emissions control system, the anticipated VOM concentration at the emissions control system exhaust is 50 ppmv or less, as carbon, regardless of inlet concentration. If the source elects to use Method 25A under this option, the exhaust VOM concentration must be 50 ppmv or less, as carbon, and the required destruction efficiency must be met for the source to have demonstrated compliance. If the Method 25A test results show that the required destruction efficiency apparently has been met, but the exhaust concentration is above 50 ppmv, as carbon, a retest is required. The retest shall be conducted using either Method 25 or Method 25A. If the retest is conducted using Method 25A and the test results again show that the required destruction efficiency apparently has been met, but the exhaust concentration is above 50 ppmv, as carbon, the source must retest using Method 25;

D) During testing, the cleaning equipment shall be operated at representative operating conditions and flow rates.

d) An owner or operator using an emissions control system other than an afterburner or carbon adsorber shall conduct testing to demonstrate compliance with the requirements of Section 219.901(d) as set forth in the owner's or operator's plan approved by the Agency and USEPA pursuant to Section 219.901(d)(3).

(Source: Amended at 35 Ill. Reg. 13676, effective July 27, 2011)