**Section 228.135 Preclude Exposure to Circulating Air**

Asbestos-containing material applied in the construction, alteration or repair of a structure shall be coated with a sealant, provided with a cover or installed in some other manner so as to preclude emission of the asbestos-containing material to the circulating air. Any plenum or other structure coated with or containing asbestos-containing insulation and used in the circulation of air in a building shall be thoroughly cleaned of all debris and waste insulation.