**Section 240.152 Steady-State Idle Mode Vehicle Exhaust Emission Standards**

a) Exhaust emissions from light duty vehicles shall not exceed the following limitations:

|  |  |  |
| --- | --- | --- |
| Model Year | Carbon Monoxide | Hydrocarbons as Hexane |
| (%) | (ppm) |
| 1996 and newer | 1.2 | 220 |

b) Exhaust emissions from light duty trucks 1 and light duty trucks 2 shall not exceed the following limitations:

|  |  |  |
| --- | --- | --- |
| Model Year | Carbon Monoxide | Hydrocarbons as Hexane |
| (%) | (ppm) |
| 1996 and newer | 1.2 | 220 |

c) Exhaust emissions from heavy duty vehicles shall not exceed the following limitations:

|  |  |  |
| --- | --- | --- |
| Model Year | Carbon Monoxide | Hydrocarbons as Hexane |
| (%) | (ppm) |
| 1996 and newer | 3.0 | 300 |

(Source: Amended at 35 Ill. Reg. 5552, effective March 18, 2011)