**Section 307.3603 Rolled Glass Manufacturing**

a) Applicability. This Section applies to discharges resulting from the process in which several mineral ingredients (sand, soda ash, limestone, dolomite, cullet, and other ingredients) are mixed, melted in a furnace, and cooled by rollers to form rolled glass.

b) Specialized Definitions. The Board incorporates by reference 40 CFR 426.31 (2003). This incorporation includes no later amendments or editions.

c) Existing Sources

1) The Board incorporates by reference 40 CFR 426.34 (2003). This incorporation includes no later amendments or editions.

2) No person subject to the pretreatment standards incorporated by reference in subsection (c)(1) may cause, threaten, or allow the discharge of any contaminant to a POTW in violation of those standards.

d) New Sources

1) The Board incorporates by reference 40 CFR 426.36 (2003). This incorporation includes no later amendments or editions.

2) No person subject to the pretreatment standards incorporated by reference in subsection (d)(1) may cause, threaten, or allow the discharge of any contaminant to a POTW in violation of those standards.

3) "New source" means any building, structure, facility, or installation whose construction commenced after October 17, 1973.

(Source: Amended at 47 Ill. Reg. 4662, effective March 23, 2023)