**Section 307.4005 Papergrade Sulfite**

a) Applicability. This Section applies to discharges resulting from: the integrated production of pulp and paper at papergrade sulfite mills where blow pit pulp washing techniques are used; and the integrated production of pulp and paper at papergrade sulfite mills where vacuum or pressure drums are used to wash pulp.

b) Specialized Definitions. The Board incorporates by reference 40 CFR 430.51 (2003). This incorporation includes no later amendments or editions.

c) Existing Sources

1) The Board incorporates by reference 40 CFR 430.56 (2003). This incorporation includes no later amendments or editions.

2) No person subject to the pretreatment standards incorporated by reference in subsection (c)(1) may cause, threaten, or allow the discharge of any contaminant to a POTW in violation of those standards.

d) New Sources

1) The Board incorporates by reference 40 CFR 430.57 (2003). This incorporation includes no later amendments or editions.

2) No person subject to the pretreatment standards incorporated by reference in subsection (d)(1) may cause, threaten, or allow the discharge of any contaminant to a POTW in violation of those standards.

3) "New source" means any building, structure, facility, or installation whose construction commenced after January 6, 1981.

(Source: Amended at 47 Ill. Reg. 4662, effective March 23, 2023)