SUBPART F: MASS LOADING LIMITS