**Section 364.204 F2 Factor**

F2 is a factor which evaluates the adequacy of existing facilities for treating the existing wastewater load to design levels. It is calculated as follows:

|  |  |  |
| --- | --- | --- |
| F2 | = | PE BOD, (existing wastewater load, industrial and domestic) |
| PE BOD, existing design capacity |

|  |  |  |
| --- | --- | --- |
| x | daily average flow, existing load | +1 |
| daily average flow, existing design capacity |