**Section 374.207 Marked Sewer Lines**

Where polyvinyl chloride (PVC) pressure mains are to be installed in the vicinity of similar water supply lines, the sewer line should be clearly marked to prevent possible future cross-connections.

(Source: Amended at 21 Ill. Reg. 12439, effective August 28, 1997)