**Section 405.112 Mine Entrances**

Bore holes, openings, drill holes, entrances to underground mines, and auger or punch mine entries must be plugged and sealed to the extent necessary to avoid the threat of water pollution.

(Source: Amended at 43 Ill. Reg. 11606, effective September 25, 2019)