SUBPART F: REQUIREMENTS FOR WELLS INJECTING HAZARDOUS WASTE