**Section 721.276 Special Requirements for Ignitable or Reactive Hazardous Secondary Material**

Containers holding ignitable or reactive hazardous secondary material must be located at least 15 meters (50 feet) from the facility's property line.

(Source: Added at 40 Ill. Reg. 11367, effective August 9, 2016)