**Section 724.329 Special Requirements for Ignitable or Reactive Waste**

Ignitable or reactive waste must not be placed in a surface impoundment, unless the waste and impoundment satisfy all applicable requirements of 35 Ill. Adm. Code 728 and the following:

a) The waste is treated, rendered, or mixed before or immediately after placement in the impoundment so that the following is true:

1) The resulting waste, mixture, or dissolution of material no longer meets the definition of ignitable or reactive waste under 35 Ill. Adm. Code 721.121 or 721.123; and

2) Section 724.117(b) is complied with;

b) The waste is managed in such a way that it is protected from any material or conditions that may cause it to ignite or react; or

c) The surface impoundment is used solely for emergencies.

(Source: Amended at 27 Ill. Reg. 3725, effective February 14, 2003)