SUBPART D: CRITERIA AND STANDARDS APPLICABLE

TO CLASS III INJECTION WELLS