SUBPART F: CRITERIA AND STANDARDS APPLICABLE

TO CLASS V INJECTION WELLS