**Section 730.169 Reporting Requirements**

Reporting requirements must, at a minimum, include the following:

a) Quarterly reports to the Agency containing the following information:

1) The maximum injection pressure;

2) A description of any event that exceeds operating parameters for annulus pressure or injection pressure as specified in the permit;

3) A description of any event that triggers an alarm or shutdown device required pursuant to Section 730.167(f) and the response taken;

4) The total volume of fluid injected;

5) Any change in the annular fluid volume;

6) The physical, chemical, and other relevant characteristics of injected fluids; and

7) The results of monitoring prescribed pursuant to Section 730.168; and

b) Reporting, within 30 days or with the next quarterly report, whichever comes later, the results of any of the following activities:

1) Periodic tests of mechanical integrity;

2) Any other test of the injection well conducted by the permittee if required by permit condition; and

3) Any well workover.

BOARD NOTE: Derived from 40 CFR 146.69 (2005).

(Source: Amended at 31 Ill. Reg. 1281, effective December 20, 2006)