**Section 160.130 Piping – Runs**

Piping shall be run as directly as possible and proper allowance made for expansion and contraction.