**Section 160.170 Piping – Tests**

After installation, piping shall be tested at a pressure fifty per cent in excess of the working pressure for thirty minutes and must be proven leak proof.

(Source: Amended at 9 Ill. Reg. 10012, effective October 1, 1985)