**Section 160.360 Tank Car Unloading Operations – Other Restrictions**

a) All connections between tank cars and pipe lines shall be in good condition and not permit leakage.

b) Tank cars shall not be left connected to pipe lines except when loading or unloading is going on, and during all such times a person shall be present and in charge.

c) The presence of flame lanterns, flame switch lights or other exposed flame lights or fires during the process of loading or unloading is prohibited.

(Source: Amended at 9 Ill. Reg. 10012, effective October 1, 1985)