**Section 251.100 Pre-Engineered Fire Suppression Systems**

a) Pre-engineered fire suppression systems may only be installed, maintained, repaired, recharged, hydro-tested, serviced, inspected and replaced by a licensed Class B distributor/Class 2 licensed employee, except as otherwise specified in this Section.

b) Licensed Class A distributors/Class 1 licensed employees may perform recharging and hydro-testing functions enumerated in Section 251.90(e) on pre-engineered fire suppression systems.

c) Pre-engineered fire suppression systems that are pre-piped in a hood and duct or other modular assembly and shipped to a location in Illinois shall be completed and certified by a licensed Class B distributor/Class 2 licensed employee.

d) Pre-engineered fire suppression systems must be installed, maintained, repaired, recharged, hydro-tested, serviced, inspected and replaced in accordance with NFPA 96, 17 and 17A, incorporated by reference in Section 251.25.