**Section 200.700 Requirements for Type 3 Magazines**

a) Type 3 magazines are intended only for the temporary containment of explosive materials and are authorized for storage only during transport to, and use at, the blast area. A storage certificate is not required for a Type 3 magazine.

b) Type 3 magazines containing explosive materials must be attended at all times. For the purposes of this subsection, "attended at all times" means that the magazine must always be within the line of sight of, and visible to, a member of the work or blasting crew authorized to enter the magazine. Pursuant to ATF Rulings 2009-3 and 2019-1, this subsection does not apply to law enforcement.

c) Type 3 magazines must be locked during transport to and from the permanent magazine and blast area except during continuous drilling and loading at the site. The requirements that Type 3 magazines be locked as specified in this subsection are in addition to the requirements that Type 3 magazines be attended at all times.

d) Daily, at the conclusion of blasting operations, all explosive materials shall be returned to a Type 1, 2, 4 or 5 magazine, as appropriate, for unattended storage.

e) All regulated explosives that are in a Type 3 magazine and/or at a blast/display site or any other site, and that are not being stored in a Department certified explosive storage magazine, must be attended at all times.

f) Type 3 magazines and blast zones shall be posted with warning signs in accordance with Section 200.701(a).

(Source: Amended at 45 Ill. Reg. 4490, effective March 26, 2021)