**Section 225.40 Transportation of Permissible Explosives from Surface to Section Magazines**

a) Any person transporting permissible explosives underground or transporting electric detonators underground must transport them in locked, acceptable container.

b) Permissible explosives and/or electric detonators may not be transported in the same transportation vehicle with tools, supplies, or more than three people.

c) If permissible explosives and detonators are transported in the same acceptable container then the permissible explosives and detonators shall be separated by at least a four inch partition made of nonsparking material.