**Section 225.47 Inventory**

a) At the beginning of each shift, the shot firer must record the quantity of:

1) permissible explosives; and

2) electric detonators

stored in that section magazine.

b) At the end of each shift, the shot firer must reconcile the quantity of permissible explosives and electric detonators used on that shift with the number of permissible explosives and electric detonators recorded as a result of the inventory which Subsection (a) requires.

c) If after the inventory required in Subsections (a) and (b), the shot firer notes a shortage of permissible explosives then, the shot firer's supervisor shall be immediately advised.