**Section 240.1350 Casing and Protective Work**

a) Whenever the rules require a mine string to be set in a mine area, the casing used inside the mine string shall be new.

b) Any protective work required in a mine area shall be under the supervision of the Mining Board.

(Source: Recodified from Section 240.850 at 15 Ill. Reg. 8566)