**Section 245.820 Secondary Containment Inspections**

*No more than one hour before initiating any stage of the high volume horizontal hydraulic fracturing operations, all secondary containment* required pursuant to Section 245.825(b) *must be visually inspected* by the permittee or the contractor performing the HVHHF operations on behalf of the permittee *to ensure* that *all structures and equipment are in place and in proper working order. The results of this inspection must be recorded and documented by the* permittee or the contractor performing the HVHHF operations on behalf of the permittee on a form prescribed by the Department, maintained in the well file, *and* made *available* at the well site *to the Department upon request*. (Section 1-75(c)(13) of the Act)