**Section 330.3960 Exit and Fire Escape Lights and Directional Signs**

Every existing facility shall meet the following requirements:

a) Standard illuminated exit lights on a separate electric circuit shall be provided at all exits on each floor. The signs shall bear the word "EXIT" in conspicuous lettering on a contrasting background to comply with local ordinances or practice. These lights shall be kept lighted at all times. (A, B)

b) A fire escape sign shall be placed over the inside of each door to the fire escape. The sign shall bear the words "FIRE ESCAPE" in conspicuous lettering on a contrasting background to comply with local ordinances or practice. These lights should be lighted at all times. (A, B)

c) White lights shall be provided on the outside of the building over each door to the fire escape. These lights shall be kept on a separate circuit and shall be kept lighted at all times unless they are on a timer or solar device. (A, B)

d) Directional signs of similar construction as above shall be provided throughout the building and its corridors as needed or required to show the direction to exits.

(Source: Amended at 13 Ill. Reg. 6562, effective April 17, 1989)