**Section 760.1060 Handwashing Facility Faucets**

Each handwashing facility shall be provided with hot and cold water tempered by means of a mixing valve or combination faucet. Any self-closing, slow-closing, or metering faucet used shall be designed to provide a flow of water for at least 15 seconds without the need to reactivate the faucet. Steam mixing valves are prohibited at handwashing facilities.