**Section 760.1330 General - Lighting**

a) Permanently fixed artificial light sources shall be installed to provide at least 20 foot candles of light on all food preparation surfaces and at warewashing work levels.

b) Permanently fixed artificial light sources shall be installed to provide, at a distance of 30 inches from the floor:

1) At least 20 foot candles of light in sales areas, utensil and equipment storage areas, and in handwashing and toilet areas; and

2) At least 10 foot candles of light in walk-in refrigeration units, dry food storage areas, and in all other areas.