**Section 785.548 Automatic Sampling Device**

If automatic sampling devices are used, they shall be constructed in such a manner as to prevent contamination of the product, and all parts must be readily accessible for cleaning in accordance with 3-A Sanitary Standards.