**Section 785.650 Starter Vats**

Bulk starter vats shall be of stainless steel or equally corrosion-resistant metal and constructed according to applicable 3-A Sanitary Standards. The vats shall be in good repair, equipped with tight-fitting lids, and have temperature controls.