**Section 785.740 Starter Vats**

Bulk starter vats shall be of stainless steel or equally corrosion-resistant metal and shall be in good repair, equipped with tight-fitting lids and have adequate temperature controls such as valves, indicating and/or recording thermometers. New vats shall be constructed according to the applicable 3-A Sanitary Standards.

(Source: Adopted at 11 Ill. Reg. 2356, effective February 1, 1987)