**Section 785.770 Rindless Cheese Press**

The press used to heat seal the wrapper applied to rindless cheese shall have square interior corners, reasonably smooth interior surface and have controls that shall provide uniform pressure and heat equally to all surfaces.

(Source: Adopted at 11 Ill. Reg. 2356, effective February 1, 1987)