**Section 785.1030 Batch or Continuous In-Containers Sterilizers**

Shall be equipped with accurate temperature controls and effective valves of regulating the sterilization process. The equipment shall be maintained in such a manner as to assure control of the length of time of processing, and to minimize the number of damaged containers.

(Source: Adopted at 11 Ill. Reg. 2356, effective February 1, 1987)