**Section 795.160 Additional Requirements for Stand-Up Booths**

a) There shall be physical barriers or other methods, such as handrails or floor markings, to indicate the proper exposure distance between ultraviolet lamps and the consumer's skin.

b) The construction of the booth shall be such that it will withstand the stress of use.

c) Access to the booth shall be of rigid construction; doors shall open outwardly. Handrails for the consumer to grasp during operation of the tanning equipment shall be provided; non-slip floors shall be provided.