**Section 800.540 Sewer Risers**

Sewer risers and laterals serving individual camp spaces shall be at least four inches inside diameter (I.D.) water tight piping. Risers at unoccupied spaces shall be sealed with a tight-fitting cap or plug.

(Source: Amended at 10 Ill. Reg. 11076, effective July 1, 1986)