**Section 800.550 Sewage Collection Systems**

Sewage collection systems shall be installed with a minimum slope of one percent. Sewage lines shall be a minimum of four inches inside diameter. In recreational areas operated during freezing weather, sewers shall be installed below the established frost line.

(Source: Amended at 10 Ill. Reg. 11076, effective July 1, 1986)